;=========================================================================================================================
;
;  GeneralTouch Touchscreen USB interface 
;
;  USB Touchscreen driver for Windows 2000/XP.
;
;  ReadMe file for touchscreen driver package
;
;  Release 2.1
;
;  Copyright 1998-2004,General Touch Technology Co., Ltd. all rights reserved.
;
;=========================================================================================================================

The GeneralTouch Touchscreen USB interface driver package for Windows 2000 and XP
contains a HID (Human Interface Device) filter driver designed for Windows using 
the WDM (Windows Driver Model) architecture, calibration program, uninstall utility, 
and a 32-bit control panel.


==================================
Supported Touchscreen controller
==================================

	- GeneralTouch PnP-compliant usb controller 2038,4001u 
	
  	 --------------------------------------------------------
  	|                                                        |
  	|  This driver does not support GeneralTouch serial      |
	|  controller 2036,2037,4001s,4001s-M.			 |
  	|                                                        |
  	|  Refer to www.Generaltouch.com for availability of	 | 
	|  drivers for these products.                           |
  	|                                                        |
   	--------------------------------------------------------

==============================
CONTENTS
==============================
1.Install/Uninstall Manual
  1.1 Installing touchscreen driver for Windows 2000/XP
  1.2 Change touchscreen settings
  1.3 Uninstall touchscreen software
  1.4 Release Notes	
2.Software package component
3.Problem solution

==============================
1.	Install/Uninstall Manual
==============================

1.1 Installing touchscreen driver for Windows 2000/XP

Note to Windows 2000/XP users: you must have administrator access rights on 
your Windows 2000/XP system to install this software. You must also have 
administrator access rights to run the touchscreen control panel and 
calibration applications.

Shutdown your computer and connect your touchscreen as described
in the accompanying documentation.

A. If Windows STARTS the New Hardware Wizard
--------------======------------------------

   1. Choose Next. Select "Search for the best driver for
      your device (Recommended)" and Choose Next.

   2. When a list of search locations is displayed, place a
      checkmark on the floppy drive containing this USB driver
      for Windows disk. Insert the disk into your floppy drive.
      (If the driver files have been copied to your hard drive or
      have been distributed on CD, place a checkmark on "Specify
      a location" and use Browse to select the directory
      containing the driver files.)

   3. Choose Next. Once the GeneralTouch Touchscreen USB
      Interface driver has been detected choose Next again.

   4. Wait while driver files are copied to your computer. Insert
      your Windows CD if prompted.

   5. Choose Finish. 

B. If Windows DOES NOT START the New Hardware Wizard
--------------==============------------------------
 
   1. After Windows loads, click the "Start" button, and then 
      click "Control Panel", "System", "Device Manager". 

   2. In the Device Manager, right click on the USB Human 
      Interface Device, and then click on Properties, Driver 
      tab, Update Driver, Next. Select "Search for the best driver 
      for your device (Recommended)" and Choose Next.

   3. When a list of search locations is displayed, place a
      checkmark on the floppy drive or CD containing this USB driver
      for Windows disk. Insert the disk into your drive. (If the 
      driver files have been copied to your hard drive, place a
      checkmark on "Specify a location" and use Browse to select 
      the directory containing the driver files.)

   4. Choose Next. Once the GeneralTouch Touchscreen USB
      Interface driver has been detected choose Next again.

   5. Wait while driver files are copied to your computer. Insert
      your Windows CD if prompted.

   6. Choose Finish. 

   7. The touchscreen calibration application, GenCalib.exe, must be used 
      manually to align cursor movement with point of touch.

=========================================
1.2	Change Touchscreen settings
=========================================

1. Click the "Start" button, point to "Settings", and then click
   "Control Panel".

2. Double-click the "GeneralTouch Touchscreen" icon,now you can change 
   your touchscreen settings, For more information about touchscreen
   settings,you can use context_sensitive help.

=========================================
1.3 	Uninstalling touchscreen driver for Windows 2000/XP.
=========================================

1. Click the "Start" button, point to "Settings", and then click
   "Control Panel".

2. Double-click the "Add/Remove Programs" icon.

3. Select "GeneralTouch Touchscreen USB interface for 2000/XP" from 
   the list of uninstallable programs on the "Install/Uninstall" tab.

4. Click the "Add/Remove" button then follow the directions on
   your screen.

===============================
1.4	Release Notes
===============================

- Because your GeneralTouch Touchscreen USB interface controller conforms to the USB HID 
  class specification, Windows 2000/XP supports it inherently with default HID class 
  drivers. You may notice that a touch will move the Windows cursor even before you install 
  this device driver package for Windows.

  However, you must install this driver package in order to install and use the calibration 
  application (used to correctly align your finger to the Windows cursor) and our
  control panel.

- Windows 2000/XP only: you must have administrator access rights to
  run the GeneralTouch Touchscreen control panel and calibration
  applications.

===============================
2. 	Software package component
===============================

Our touchscreen USB interface driver software package is composed of the following programs:

          GenUsb.Sys                 Our touchscreen USB driver(using WDM architecture)

	  GenUsbXp.Inf	  	     Our touchscreen HID interface INF file

          GenTouch.Cpl               32 bit Touchscreen control panel.

	  UnInst.exe		     32 bit Touchscreen uninstall utility.	

          GenCalib.exe               32 bit Touchscreen calibration program.

	  GenUsb.hlp		     context_sensitive help file.

	  Null.cur		     null cursor.
     
          README.txt                 It's me!


==============================
3.	Problem solution
==============================

-  Make sure that your USB host controller and root hub is available before installation,
   some mainboard can disable usb function in CMOS setup,you should enable it and install default
   driver for it.

;==================================================================================================================
;
;		Copyright 1998,2001 General Touch Technology Co., Ltd. All rights reserved.
;
;                                (http://www.GeneralTouch.com)
;
;==================================================================================================================
