TG558 driver package for Custom Engineering Spa Custom TG558 printer:

Windows 2000.
Windows XP.
Windows 2K3.

Installation procedure:

Serial, parallel and network interface
For (W2K, XP, W2K3) you must execute the standard printer installation procedure.

USB interface
Follow the automatic wizard procedure.

This driver supports some kind of printers:
"Custom TG558 35 mm" and "Custom TG558 58 mm"

Every printer supports some page format:


"Custom TG558 35 mm"

 "Tg558 35 mm  Roll Short" (Default)
 "Tg558 35 mm  Roll"       
 "Tg558 35 x 58 mm"
 "Tg558 35 x 85 mm"
 "Tg558 35 x 116 mm"
 "Tg558 35 x 174 mm"       
 "Tg558 35 x 232 mm"



"Custom TG558 58 mm"

 "Tg558 58 mm  Roll Short" (Default)
 "Tg558 58 mm  Roll"       
 "Tg558 58 x 58 mm"
 "Tg558 58 x 85 mm"
 "Tg558 58 x 116 mm"
 "Tg558 58 x 174 mm"       
 "Tg558 58 x 232 mm"



If the system driver properties section shows these pages format and other not here
specified, you must select only the above mentioned pages format.
