Driver package for CUSTOM ENGINEERING TG2480 printer model

OS Supported:

Windows 2000.
Windows XP.
Windows 2K3.

Installation procedure:

Serial interface
For (W2K, XP, W2K3) you must execute the standard printer installation procedure.

USB interface
Follow the automatic wizard procedure.

This driver supports some kind of printer:
"Custom TG2480"

The "TG2480" can prints on a paper width size of 80mm.

The "TG2480" printer supports some page format:

"TG2480 PTP" special page: see note below
"TG2480 Roll Short"
"TG2480 Roll"
"TG2480 80 x 80 mm"
"TG2480 80 x 120 mm"
"TG2480 80 x 180 mm"
"TG2480 80 x 240 mm"

[ the defalut installation page is "TG2480 PTP" ]


If the system driver properties section shows these pages format and other not here
specified, you must select only the above mentioned pages format.


Note for "TG2480 PTP"
This pages must be used only for the "Printer Test Page" (PTP) operation.
Don't use this page to print out from applications.